CMSIS-RTOS: Revision History

| CMSIS-RTOS Version 1.02 CMSIS-RTOS API: Generic RTOS interface for Cortex-M processor-based devices.

- Main Page
- Usage and Description
- Reference

Revision History

Version | Description
--- | ---
V1.02 - only documentation changes | Added: Overview of the CMSIS-RTOS Validation Software Pack. Clarified: Behaviour of Timout Value.
V1.02 | Added: New control functions for short timeouts in microsecond resolution osKernelSysTick, osKernelSysTickFrequency, osKernelSysTickMicroSec. Removed: osSignalGet.
V1.01 | Added capabilities for C++, kernel initialization and object deletion. Prepared for C++ class interface. In this context to const attribute has been moved from osXxxxDef_t typedefs to the osXxxxDef macros. Added: osTimerDelete, osMutexDelete, osSemaphoreDelete.
Added: osKernelInitialize that prepares the Kernel for object creation.
V1.00 | First official Release. Added: osKernelStart; starting 'main' as a thread is now an optional feature. Semaphores have now the standard behavior. osTimerCreate does no longer start the timer. Added: osTimerStart (replaces osTimerRestart). Changed: osThreadPass is renamed to osThreadYield.
V0.02 | Preview Release.